路由器连接：

Show ip route

Conf t

Int f0/0

No ip address

Ip address 1.1.1.100 255.255.255.0

No shutdown

